Instructions: Answer each question by marking true or false according to the information given in the presentation. Additionally, if the answer is false, modify the sentence to make it become true.

|  |  |  |
| --- | --- | --- |
| EX.  The 5 most common excavation hazards are; cave-ins, falls & falling loads, mobile equipment, hazardous atmosphere, and ~~dog bites~~.  hitting utility lines | True | False |
| 1. A competent person can classify soil, inspect protective systems, design structural ramps, monitor water removal equipment, and conducting daily site inspections. | True | False |
| 2. There are 4 soil classifications; stable rock, Type A soil, Type B Soil, and Type AB soil. | True | False |
| 3. There must be a safe means of exit every 25 feet in an excavation greater than 4 feet. | True | False |
| 4. Wear reflective vests to make yourself more visible to operators | True | False |
| 5. Call 811 to have utilities located by local companies | True | False |
| 6. A trench is a narrow underground excavation no wider than 15 feet. | True | False |
| 7. Sloping, Shoring, and Shielding are protective systems used for trenching and excavation | True | False |
| 8. The atmosphere in the confined space must be initially and continuously tested using air monitoring equipment. | True | False |
| 9. Weekly inspections of excavations, the adjacent areas, and protective systems shall be made by a competent person. | True | False |
| 10. Materials/Equipment without protective systems must be at least 6 inches from the edge of excavations. | True | False |

|  |  |  |
| --- | --- | --- |
| EX.  The 5 most common excavation hazards are; cave-ins, falls & falling loads, mobile equipment, hazardous atmosphere, and dog bites.  hitting utility lines. | True | False |
| 1. A competent person can classify soil, inspect protective systems, design structural   ramps, monitor water removal equipment, and conducting daily site inspections. | True | False |
| 2. There are 4 soil classifications; stable rock, Type A soil, Type B Soil, and Type AB  soil.  Type C soil | True | False |
| 3. There must be a safe means of exit every 25 feet in an excavation greater than 4  feet. | True | False |
| 4. Wearing reflective vests to make yourself more visible to operators. | True | False |
| 5. Call 811 to have utilities located by local companies. | True | False |
| 6. A trench is a narrow underground excavation no wider than 15 feet. | True | False |
| 7. Sloping, Shoring, and Shielding are protective systems used for trenching and  excavation. | True | False |
| 8. The atmosphere in the confined space must be initially and continuously tested using air monitoring equipment. | True | False |
| 9. Weekly inspections of excavations, the adjacent areas, and protective systems shall be made by a competent person.  Daily | True | False |
| 10. Materials/Equipment without protective systems must be at least 6 inches from the edge of excavations.  2 feet | True | False |