Trainee Name: Score: /10

Crane Safety Retention Quiz

Note: Multiple Choice, true/ false, Circle Most Appropriate Answer

1. Which is not a common hazard associated with cranes?
2. Overloading B) Power lines C) Improper ground conditions D) Rust on the bumper
3. Which is not a common maintenance hazard with cranes
4. Damage to wire rope B) Alignment Issues C) Bent/ damaged hooks D) Chipped Paint
5. How far does the clearance from power lines need to be?
6. 10ft B) 20ftC) 30ft D) 40ft
7. Which is not a type of overload protection system?
8. Mechanical B) Electrical C) Industrial D) Chain hoist
9. What is a weather condition to be aware of before operating a crane?
10. Lightning B) Light rain C) Light wind D) Heavy sunlight
11. Which is not a setup hazard involving cranes
12. Ground is level B) When checking outriggers, there should be floatC) Large enough area to satisfy cranes radii D) outriggers are extended properly
13. Outriggers should never be…
14. Extended into a person B) Extended properly C) Flat D) Centered on the surface
15. How often is a periodic inspection?
16. 1-3 Months B) 4-6 Months C) 8-10 Months D) 1-12 Months

True/False

1. A crane must contact a power line for there to be an accident.

True False

1. Objects slipping/ falling from a crane is not only harmful to people, but the property around it.

True False

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Trainee Signature Trainer Signature

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Date: Date:

Answer Key:

1. D
2. D
3. B
4. C
5. A
6. B
7. A
8. D
9. False
10. True